[15] INTAKE AND EXHAUST - - ON-VEHICLE SERVICE - WASTE GATE ACTUATOR CHECK <Turbo> | PRINT PAGE / INDEX / PRIOR / NEXT

| WASTE GATE ACTUATOR CHECK <Turbo>
| Connect a manual pump (pressure-application type) to nipple. CAUTION In order to avoid damage to the diaphragm, do not apply a pressure of 60 kPa or higher. While gradually applying pressure, check the pressure that begins to activate (approximately 1 mm stroke) the waste gate actuator rod. Standard value: Approximately 80 kPa If there is a significant deviation from the standard value, check the actuator or the waste gate valve: replace actuator or turbocharger assembly if necessary.

[15] INTAKE AND EXHAUST - - ON-VEHICLE SERVICE - WASTE GATE ACTUATOR CHECK <Turbo> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation