[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - TROUBLESHOOTING - MUT-II/III FLIGHT RECORDER FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

| MUT-II/III FLIGHT RECORDER FUNCTION The SWS monitor cartridge memory can store the ECU check results, the service data, the communication data obtained by the function diagnosis. This communication data can be displayed as a chart or graphical form. If data obtained by the flight recorder function has to be stored for long time, the data can be transferred to the SWS monitor cartridge. By doing this, you can disconnect the MUT-II/III to prevent excessive battery drain. NOTE: For the details about the MUT-II/III flight recorder function, refer to MUT-II reference manual or MUT-III user’s manual.

[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - TROUBLESHOOTING - MUT-II/III FLIGHT RECORDER FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation