[23A] AUTOMATIC TRANSMISSION (FF) - - A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS - REMOVAL AND INSTALLATION <VEHICLES WITH RHD> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <VEHICLES WITH RHD>
WARNING When removing and installing the shift lock cable unit, be careful not to hit it against the SRS-ECU.
Pre-removal and Post-installation Operation Selector Lever Assembly Removal and Installation (Refer to .) Instrument Lower Panel Removal and Installation (Refer to GROUP 52A - Instrument Panel .) Lower Column Cover Removal and Installation (Refer to GROUP 37 - Steering Shaft .) Key Interlock and Shift Lock Mechanisms Check <after installation only> (Refer to .)
|  |  | Removal steps
--- | --- | --- | ---
<<A>> | >>B<< | 1. | Key interlock cable connection (steering lock cylinder side)
|  | • | Footrest
|  | 2. | Shift lock cable connection (brake pedal side)
| >>A<< | 3. | Shift lock cable unit
| REMOVAL SERVICE POINTS
| <<A>> KEY INTERLOCK CABLE (STEERING LOCK CYLINDER SIDE) REMOVAL Turn the ignition switch to the ACC position and then pull the key interlock cable out from the ignition key cylinder.
| INSTALLATION SERVICE POINTS
| >>A<< SHIFT LOCK CABLE UNIT INSTALLATION Shift the selector lever to the P position and turn the ignition switch to the LOCK (OFF) position.
| After installing the rod of the shift lock cable unit to the lock cam of the selector lever assembly, tighten the bolts of the shift lock cable unit to the specified torque. Tightening torque: 5.0 ± 1.0 N·m Check the operation of the selector lever. (Refer to .)
| >>B<< KEY INTERLOCK CABLE (STEERING LOCK CYLINDER SIDE) INSTALLATION Turn the ignition switch to the ACC position and then install the key interlock cable to the ignition key cylinder.

[23A] AUTOMATIC TRANSMISSION (FF) - - A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS - REMOVAL AND INSTALLATION <VEHICLES WITH RHD> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation