[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SYMPTOM PROCEDURES - Inspection Procedure 3: Throttle Valve will not Fully Open or Close <4G69-R.H. drive vehicles> | PRINT PAGE / INDEX / PRIOR / NEXT

Inspection Procedure 3: Throttle Valve will not Fully Open or Close <4G69-R.H. drive vehicles>
DIAGNOSIS PROCEDURE
STEP 1. Check the MUT-II/III diagnosis code Q: Is any diagnosis code set? YES: Refer to GROUP 13C, Troubleshooting - Inspection Chart for Diagnosis Code . NO: Go to Step 2.
STEP 2. Retest the system. Q: Does the throttle valve fully open and close? YES: The procedure is complete. NO: Return to Step 1.

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SYMPTOM PROCEDURES - Inspection Procedure 3: Throttle Valve will not Fully Open or Close <4G69-R.H. drive vehicles> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation