[42] BODY - - TAILGATE - TAILGATE HANDLE AND LATCH - ]INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| ]INSPECTION
| TAILGATE LOCK ACTUATOR CHECK
LEVER POSITION | BATTERY CONNECTION | LEVER OPERATION
--- | --- | ---
At the "LOCK" position | Connect terminal No.1 and the negative battery terminal. Connect terminal No.2 and the positive battery terminal. | The lever moves from the "LOCK" position to the "UNLOCK" position.
At the "UNLOCK" position | Connect terminal No.2 and the negative battery terminal. Connect terminal No.1 and the positive battery terminal. | The lever moves from the "UNLOCK" position to the "LOCK" position.
| TAILGATE LATCH SWITCH CHECK <VEHICLES WITH KEYLESS ENTRY SYSTEM>
LEVER POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
At the "LOCK" position | 1 - 2 (Earth) | Open circuit
At the "UNLOCK" position | 1 - 2 (Earth) | Less than 2 ohms

[42] BODY - - TAILGATE - TAILGATE HANDLE AND LATCH - ]INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation