[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - CRANKSHAFT POSITION SENSOR - REMOVAL AND INSTALLATION <4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G6-DOHC>
Pre-removal and Post-installation Operation Timing Belt Removal and Installation (Refer to GROUP 11C, Timing Belt .)
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Power steering pressure switch connector
|  | 2. | A/C compressor connector
|  | 3. | A/C compressor connector clamp
<<A>> |  | 4. | Power steering oil pump assembly
|  | 5. | Power steering oil pump bracket
|  | 6. | Crankshaft position sensor
|  | 7. | Crankshaft position sensor connector bracket
| REMOVAL SERVICE POINT
| <<A>> POWER STEERING OIL PUMP ASSEMBLY REMOVAL Remove the power steering oil pump assembly from the bracket with the hose attached. NOTE: Place the removed power steering oil pump assembly in a place where it will not be a hindrance when removing and installing and secure it with a cord or wire.

[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - CRANKSHAFT POSITION SENSOR - REMOVAL AND INSTALLATION <4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation