[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - A/T CONTROL COMPONENT CHECK - A/T CONTROL RELAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| A/T CONTROL RELAY CHECK
| Removal the A/T control relay.
| Use the jumper leads to connect A/T control relay terminal 2 to the negative battery terminal and terminal 3 to the positive battery terminal. Check the continuity between A/T control relay connector terminals 1 and 4 while alternately connecting and disconnecting the jumper leads from the battery terminals.
Jumper leads | Continuity between terminals 1 and 4
--- | ---
Connected | Less than 2 Ω
Disconnected | Open circuit
If there is a malfunction, replace the A/T control relay.

[23A] AUTOMATIC TRANSMISSION (FF) - - ON-VEHICLE SERVICE - A/T CONTROL COMPONENT CHECK - A/T CONTROL RELAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation