[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A9. CHECK RADIATOR HOSES FOR DAMAGE AND PROPER CONNECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| A9. CHECK RADIATOR HOSES FOR DAMAGE AND PROPER CONNECTION
| Check entire circumference and length of hoses, using a mirror as required. Check that hoses installed in grommets pass through the centre of the grommets. Check all clamps for tightness and connections for leakage.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A9. CHECK RADIATOR HOSES FOR DAMAGE AND PROPER CONNECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation