[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - TROUBLESHOOTING - IGNITION KEY REMINDER BUZZER AND DOOR LOCK PREVENTION FUNCTION DIAGNOSIS | PRINT PAGE / INDEX / PRIOR / NEXT

TROUBLESHOOTING

IGNITION KEY REMINDER BUZZER AND DOOR LOCK PREVENTION FUNCTION DIAGNOSIS The ignition key reminder tone alarms are controlled by the Smart Wiring System (SWS). For troubleshooting, refer to respective Groups below. Not using SWS monitor <Hong Kong spec.>: GROUP 54B, Troubleshooting . Using SWS monitor <Hong Kong spec.>: GROUP 54C, Troubleshooting . Not using SWS monitor <Except for Hong Kong spec.>: GROUP 54D, Troubleshooting . Using SWS monitor <Except for Hong Kong spec.>: GROUP 54E, Troubleshooting .

[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - TROUBLESHOOTING - IGNITION KEY REMINDER BUZZER AND DOOR LOCK PREVENTION FUNCTION DIAGNOSIS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation