[54A] CHASSIS ELECTRICAL - - FOG LAMP - FOG LAMP - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <2400>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Fog lamp assembly
|  | 2. | Fog lamp
<<A>> |  | 3. | Fog lamp bulb
| REMOVAL SERVICE POINT
| <<A>> FOG LAMP BULB REMOVAL CAUTION Use the specified genuine part when replacing the bulb. Do not touch the glass portion of bulb with bare hand or dirty gloves. Should the glass portion be spoiled, remove the soil as soon as possible using alcohol or thinner and let it dry before mounting.
| Turn the fog lamp bulb left to remove it.

[54A] CHASSIS ELECTRICAL - - FOG LAMP - FOG LAMP - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation