[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - GENERAL SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL SPECIFICATIONS
Transmission model | Drive system | Number of speeds | Damper clutch | Low-reverse one-way clutch | Final gear ratio
--- | --- | --- | --- | --- | ---
W5A51-3-DZB | 4WD | 5 speeds | Provided | Provided | 3.333
Item | W5A51
--- | ---
Torque converter | Type | Three-element, one-stage, two-phase
Transmission | Type | Five forward speeds, one reverse
Gear ratio | 1st | 3.789
2nd | 2.057
3rd | 1.421
4th | 1.000
5th | 0.731
Reverse | 3.865
Number of underdrive clutch discs | 4
Number of overdrive clutch discs | 4
Number of reverse clutch discs | 2
Number of direct clutch discs | 5
Number of low-reverse brake discs | 6
Number of second brake discs | 4
Transfer | Type | Constant mesh
LIST OF VALVE BODY SPRINGS
| Wire diameter mm | Coil diameter mm | Free length mm | Number of loops
--- | --- | --- | --- | ---
Regulator valve spring | 1.8 | 15.7 | 86.7 | 24
Underdrive pressure control valve spring | 0.7 | 7.6 | 37.7 | 25
Overdrive pressure control valve spring | 0.7 | 7.6 | 37.7 | 25
Low-reverse pressure control valve spring | 0.7 | 7.6 | 37.7 | 25
Second pressure control valve spring | 0.7 | 7.6 | 37.7 | 25
Reduction pressure control valve spring | 0.7 | 7.6 | 37.7 | 25
Torque converter valve spring | 1.6 | 11.2 | 34.4 | 12.5
Damper clutch control valve spring | 0.7 | 5.9 | 28.1 | 19
Fail-safe valve A spring | 0.7 | 8.9 | 21.9 | 9.5
Damping valve spring | 1.0 | 7.7 | 35.8 | 17
Line relief valve spring | 1.0 | 7.0 | 17.3 | 10
Orifice check ball spring | 0.5 | 4.5 | 17.2 | 15

[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - GENERAL SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation