[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - WINDSHIELD WIPER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

WINDSHIELD WIPER

REMOVAL AND INSTALLATION
|  |  | Wiper blade removal steps
--- | --- | --- | ---
|  | 1. | Wiper blade assembly
| >>B<< | 2. | Wiper blade
|  |  | Windshield wiper motor and link assembly removal steps
| >>A<< | 3. | Wiper arm and blade assembly
|  | 4. | Hood weather strip
|  | 5. | Roof drip moulding and front deck garnish connection
|  | 6. | Front deck garnish
|  | 7. | Windshield wiper motor and link assembly
|  | 8. | Link assembly
|  | 9. | Windshield wiper motor assembly
NOTE: For removal and installation of the wiper and washer switch, refer to GROUP 54A, Column switch .
| INSTALLATION SERVICE POINTS
| >>A<< WIPER BLADE INSTALLATION
| CAUTION For good windshield wiper wiping performance, use a passenger-side windshield wiper without an curve in the backing of the wiper blade. The windshield wiper on the driver's side should be a wiper blade with a curved backing.
| >>B<< WIPER BLADE ASSEMBLY INSTALLATION
| Install the wiper blade at the specified position (standard value). Standard value: Driver’s side (A): 30 ± 5 mm Passenger’s side (B): 65 ± 5 mm

[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - WINDSHIELD WIPER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation