[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS OUTSIDE THE VEHICLE - D6. CHECK FUEL HOSES AND PIPES FOR LEAKAGE OR DETERIORATION | PRINT PAGE / INDEX / PRIOR / NEXT

| D6. CHECK FUEL HOSES AND PIPES FOR LEAKAGE OR DETERIORATION
| Check entire circumference and length of hoses and pipes. Check all clamps for tightness and connections for leakage.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS OUTSIDE THE VEHICLE - D6. CHECK FUEL HOSES AND PIPES FOR LEAKAGE OR DETERIORATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation