[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 94: Side Impact Sensor (RH) Power Supply Circuit System | PRINT PAGE / INDEX / PRIOR / NEXT

Diagnosis code 94: Side Impact Sensor (RH) Power Supply Circuit System
OPERATION The side impact sensor includes an analog G sensor and CPU, etc. The CPU monitors the analog G sensor output signal. If the CPU judges that the side air bags should be deployed, it sends a fire signal to the SRS-ECU to deploy the side air bags. Besides that, the CPU diagnoses the internal components of the side impact sensor. If a malfunction occurs, it requests the SRS-ECU to set a diagnosis code.
DIAGNOSIS CODE SET CONDITIONS This diagnosis code is set if the power supply voltage of the side impact sensor (RH) drops below the rated value for a continuous period of 5 seconds or more. However, diagnosis code number 94 will be automatically cleared and the SRS warning lamp will switch off if the condition returns to normal.
PROBABLE CAUSES Damaged wiring harnesses or connectors Malfunction of the side air bag module (RH) (squib) Malfunction of the SRS-ECU
| DIAGNOSIS PROCEDURE
| STEP 1. Check the side impact sensor (RH) power supply circuit at the side impact sensor (RH) connector D-41. Disconnect the negative battery terminal. Disconnect side impact sensor (RH) connector D-41, and measure at the wiring harness side. Connect the negative battery terminal. Turn the ignition switch to the "ON" position.
| CAUTION Do not insert a test probe into the terminal from its front side directly as the connector contact pressure may be weakened. Measure the voltage between the D-41 harness side connector terminal 2 and body earth. OK: 9 V or more Q: Is the check result normal? YES: Replace the side impact sensor (RH) (Refer to ). Then go to Step 3. NO: Go to Step 2.
| STEP 2. Check the harness wires for open circuit or short circuit between SRS-ECU connector C-114 (terminal No.40 and 42) and side impact sensor (RH) connector D-41 (terminal No.1 and 2). Q: Are the harness wires between SRS-ECU connector C-114 (terminal No.40 and 42) and side impact sensor (RH) connector D-41 (terminal No.1 and 2) in good condition? YES: Erase the diagnosis code memory, and check the diagnosis code. If diagnosis code 94 sets, replace the SRS-ECU (Refer to ). Then go to Step 3 . NO: Repair the harness wires between SRS-ECU connector C-114 and side impact sensor (RH) connector D-41. Then go to Step 3.
| STEP 3. Check whether the diagnosis code is reset. Q: Is diagnosis code 94 set? YES: Return to Step 1. NO: The procedure is complete (If no malfunctions are found in all steps, an intermittent malfunction is suspected). Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points .

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 94: Side Impact Sensor (RH) Power Supply Circuit System | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation