[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B12. CHECK EXHAUST PIPE CONNECTIONS FOR GAS LEAKAGE, AND CHECK PIPE INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

| B12. CHECK EXHAUST PIPE CONNECTIONS FOR GAS LEAKAGE, AND CHECK PIPE INSTALLATION Confirm that the exhaust pipe does not interfere with any body components. Check the exhaust pipe for damage by stones, etc. Start the engine and check for gas leaks from the exhaust pipe connections.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B12. CHECK EXHAUST PIPE CONNECTIONS FOR GAS LEAKAGE, AND CHECK PIPE INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation