[00] GENERAL - - VEHICLE IDENTIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

VEHICLE IDENTIFICATION
| VEHICLE IDENTIFICATION CODE PLATE
| The vehicle information code plate is riveted onto the cowl top outer panel in the engine compartment. The plate shows model code, engine model, transmission model and body colour code.
No. | Item | Content
--- | --- | ---
1 | MODEL | CU5WXRMYZL | CU5W: Vehicle model
XRMYZL: Model series
2 | ENGINE | 4G69 | Engine model
3 | EXT | T12E | Exterior code
4 | TRANS AXLE | W4A4B 3312 | W4A4B:Transmission model 3312: Rear differential (a decimal point is omitted)
5 | COLOUR | W13 | W13: Body colour code
6 | INT | 56S | 56S: Interior code
7 | OPT | ZQ3 | ZQ3: Equipment code
| For monotone colour vehicles, the body colour code shall be indicated.
| VEHICLE SAFETY CERTIFICATION LABEL <GCC>
| The vehicle safety certification label is attached to the face of the left door sill. This label indicates the month and year of manufacture, Gross Vehicle Weight Rating (GVWR), front and rear Gross Axle Weight Rating (GAWR), and Vehicle Identification Number (VIN).
MODELS
FOR GENERAL EXPORT (Except for Hong Kong, Brunei, Singapore, Malaysia, Brazil, South Africa and Argentina)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU4W | XRHEZL/R | 4G64-SOHC (2,351 mL) | W4A42 <4WD, INVECS-II 4A/T> | MPI
CU5W | XRMYZL | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T>
XRHYZL
XRHJZL
(For Hong Kong, Brunei, Singapore, Malaysia)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU2W* | LRMER1D | 4G63-SOHC-Non-Turbo (1,997 mL) | F4A42 <2WD, INVECS-II 4A/T> | MPI
LYXFZR1D | 4G63-DOHC-Turbo (1,997 mL) | W5A51 <4WD, INVECS-II 5A/T>
CU5W* | XRHYZR1D | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T>
(For Brazil)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZL1F | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZL1F
(For South Africa)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZR6S | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZR6S
(For Argentina)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRHYZL6A | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
FOR GCC
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZLW | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZLW
FOR NEW ZEALAND
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU2W* | LRMER1D | 4G63-SOHC-Non-Turbo (1,997 mL) | F4A42 <2WD, INVECS-II 4A/T> | MPI
LYXFZR1D | 4G63-DOHC-Turbo (1,997 mL) | W5A51 <4WD, INVECS-II 4A/T>
CU5W | XRMYZR8 | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T>
XRHYZR8
XRXYZR8
FOR AUSTRALIA
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZR8 | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZR8
XRXYZR8
NOTE: * indicates the vehicles as "Hong Kong spec." in the running text.
MODEL CODE
No. | Items | Contents
--- | --- | ---
1 | Development | CU: MITSUBISHI AIRTREK/OUTLANDER
2 | Engine type | 2: 1,997 mL petrol engine 4: 2,351 mL petrol engine 5: 2,378 mL petrol engine
3 | Sort | W: Wagon
4 | Body style | L, X: 5-door hatchback
5 | Transmission type | R: 4-speed automatic transmission Y: 5-speed automatic transmission
6 | Trim level | H: GLS <Except for Hong Kong, Brunei, Singapore, Malaysia, New Zealand and Australia>, Sport gear <For Hong Kong, Brunei, Singapore, Malaysia>, XLS <For Australia and New Zealand> M: GLX <Except for Hong Kong, Brunei, Singapore, Malaysia, Australia and New Zealand>, 20V <For Hong Kong, Brunei, Singapore, Malaysia and New Zealand>, LS <For Australia and New Zealand> X: Turbo R <For Hong Kong, Brunei, Singapore, Malaysia and New Zealand>, LIMITED <For Australia and New Zealand>
7 | Specification engine feature | E: MPI-SOHC F: MPI-DOHC Y, J: MPI-SOHC MIVEC
8 | Special feature | None: 2WD Z: 4WD
9 | Steering wheel location | L: Left hand R: Right hand
10 | Destination | None: For General Export (Except for Hong Kong, Brunei, Singapore, Malaysia, Brazil, South Africa and Argentina) 1D: For Hong Kong, Brunei, Singapore, Malaysia and New Zealand (4G63) 1F: For Brazil 6S: For South Africa 6A: For Argentina W: For GCC 8: For Australia and New Zealand (4G69)
| CHASSIS NUMBER
| The chassis number is stamped on the toeboard inside the engine compartment.
Hong Kong spec.
No. | Item | Content
--- | --- | ---
1 | Development order | CU | AIRTREK
2 | Engine | 2 | 2.0L MPI (4G63)
4 | 2.4L MPI MIVEC (4G69)
3 | Soft | W | Station wagon
4 | Serial number | - | -
GCC (except UAE, Kuwait and Oman)
No. | Item | Content
--- | --- | ---
1 | Country | J | Japan
2 | Make | E | Mitsubishi
3 | Vehicle type | 4 | Multi-purpose passenger vehicle (MPV)
4 | Others | L | GVWR/BRAKE SYSTEM 1,814-2,268lbs/HYDRAULIC
5 | Line | S | OUTLANDER
6 | Price class | 2 | 2: S, M 5: H
7 | Body | 1 | 5-door wagon
8 | Engine | F | 2.4L MPI MIVEC (4G69)
9 | Check digits* |  | 0, 1, 2, 3, -----------9, X
10 | Model year | 5 | 4: 2005 year
11 | Plant | U | U: Mizushima
12 | Serial number |  | 000001 to 999999
| NOTE: *: Check digit means a single number, or letter X, used to verify the accuracy of transcription of vehicle identification number.
General Export, Australia and GCC-UAE, Kuwait and Oman
No. | Item | Content
--- | --- | ---
1 | Fixed figure | J | Asia
2 | Distribution channel | M | Japan channel
3 | Destination | Y | For General Export and GCC
F | For Australia
4 | Body style | X | 5-door hatchback
5 | Transmission type | R | 4-speed automatic transmission
6 | Development order | CU | AIRTREK/OUTLANDER
7 | Engine | 4 | 2,351 mL petrol engine (4G64)
5 | 2,378 mL petrol engine (4G69)
8 | Soft | W | Station wagon
9 | Model year | 5 | 2005
10 | Plant | U | Mizushima
11 | Serial number | - | -
| VEHICLES IDENTIFICATION NUMBER LOCATION
| The vehicle identification number (VIN) is located on a plate attached to the left top side of the instrument panel.
| VEHICLE IDENTIFICATION CODE CHART PLATE (GCC ONLY) All vehicle identification numbers contain 17 digits. The vehicle number is a code which tells country, make, vehicle type, etc. <Except vehicles for UAE, Kuwait and Oman>
No. | Item | Content
--- | --- | ---
1 | Country | J: Japan
2 | Make | E: Mitsubishi
3 | Vehicle type | 4: Multi-purpose passenger vehicle (MPV)
4 | Others | GVWR/BRAKE SYSTEM L; 1,814-2,268 lbs/HYDRAULIC
5 | Line | S: OUTLANDER
6 | Price class | 2: S, M
7 | Body | 1: 5-door wagon
8 | Engine | F: 2.4L MPI(4G69)
9 | Check digits* | 0, 1, 2, 3, -----------9, X
10 | Model year | 5: 2005 year
11 | Plant | U: Mizushima
12 | Serial number | 000001 to 999999
| NOTE: *: Check digit means a single number, or letter X, used to verify the accuracy of transcription of vehicle identification number. <UAE, Kuwait and Oman>
No. | Item | Content
--- | --- | ---
1 | Fixed figure | J: Asia
2 | Distribution channel | M: Japan channel
3 | Destination | Y: For GCC
4 | Body style | X: 5-door hatchback
5 | Transmission type | R: 4-speed automatic transmission
6 | Development order | CU: OUTLANDER
7 | Engine | 5: 2,378 mL petrol engine
8 | Soft | W: Station wagon
9 | Model year | 5: 2005
10 | Plant | U: Mizushima
11 | Serial number | 000001 to 999999
| ENGINE MODEL STAMPING
| The engine model is stamped on the cylinder block. These engine model numbers are as shown as follows.
Engine model | Engine displacement
--- | ---
4G63 | 1,997 mL
4G64 | 2,351 mL
4G69 | 2,378 mL
| The engine serial number is stamped near the engine model number.
| THEFT PROTECTION <FOR BRAZIL AND ARGENTINA>
LOCATIONS
Label area
THEFT PROTECTION <FOR GCC>
LOCATIONS
Label area

[00] GENERAL - - VEHICLE IDENTIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation