[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SYMPTOM PROCEDURES - Inspection Procedure 4: Accelerator Pedal Operation is not Smooth (Over Acceleration) <4G63, 4G64, 4G69-L.H. drive vehicles> | PRINT PAGE / INDEX / PRIOR / NEXT

Inspection Procedure 4: Accelerator Pedal Operation is not Smooth (Over Acceleration) <4G63, 4G64, 4G69-L.H. drive vehicles>
DIAGNOSIS PROCEDURE
STEP 1. Check the accelerator pedal. Q: Is the accelerator pedal loose? YES: Tighten the fasteners. Then go to Step 4. NO: Go to Step 2.
STEP 2. Check the accelerator cable wiring. Q: Is the accelerator cable routing bent sharply? YES: Correct the cable routing Then go to Step 4. NO: Go to Step 3.
STEP 3. Check the accelerator cable lubricant. Q: Is the accelerator cable lubricated sufficiently? YES: Go to Step 4. NO: Refill or replace the lubricant. Then go to Step 4.
STEP 4. Retest the system. Q: Does the accelerator pedal work normally? YES: The procedure is complete. NO: Return to Step 1.

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SYMPTOM PROCEDURES - Inspection Procedure 4: Accelerator Pedal Operation is not Smooth (Over Acceleration) <4G63, 4G64, 4G69-L.H. drive vehicles> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation