[54A] CHASSIS ELECTRICAL - - HEADLAMP - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

HEADLAMP

SERVICE SPECIFICATIONS
<2000>
Item | Standard value | Limit
--- | --- | ---
Headlamp aiming (Low-beam side) | Vertical direction | Within 0.24° below horizontal (H) | ± 0.29° from the standard value
Horizontal direction | Position at which the stat up point of 15° is crossed with vertical line (V) | ± 0.5° from the standard value
Headlamp aiming (High-beam side) | Vertical direction | The centre of the high-beam hot zone is at the intersection of the (H) and (V) lines. | ± 0.5° below the standard value
<2400>
Item |  | Standard value | Limit
--- | --- | --- | ---
Headlamp aiming (Low-beam side) | Vertical direction | Within 0.57° below horizontal (H) | The headlamp beam should tilt downwards by 0.17° or more.
Horizontal direction | Position at which the stat up point of 15° is crossed with vertical line (V) | -
Headlamp aiming (High-beam side) | Vertical direction | High-intensity zone centre should be within 0.42° below horizontal (H) | The headlamp beam should tilt downwards by 0.09° or more.
Horizontal direction | High-intensity zone centre should be along the vertical line (V). | The vertical headlamp beam range should be within 1°.

[54A] CHASSIS ELECTRICAL - - HEADLAMP - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation