[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - OPERATION AND FUNCTION QUICK-REFERENCE TABLE FOR INPUT SIGNAL INSPECTION PROCEDURES | PRINT PAGE / INDEX / PRIOR / NEXT

OPERATION AND FUNCTION QUICK-REFERENCE TABLE FOR INPUT SIGNAL INSPECTION PROCEDURES If troubles have occurred in the functions which use the SWS simultaneously, observe the table below to check input signals. (This table shows only the input signals which will cause troubles in at least two functions simultaneously).
Function | P-1 | P-2 | P-4 | P-5 | P-6 | P-12 | P-14 | P-15 | P-18
--- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Ignition key reminder buzzer function <Vehicles for GCC only> | - | × | × | - | - | × | - | - | -
Lamp reminder function | - | × | × | × | - | - | - | - | -
Control of central door locking | - | - | - | - | - | - | - | × | -
Key reminder function <Vehicles with keyless entry system> | - | - | × | - | - | × | - | × | -
Door locking released due to impact detection. | - | - | - | - | - | - | - | - | -
Keyless entry system | - | - | × | - | - | × | × | × | -
Keyless entry hazard warning lamp answerback | - | - | - | - | - | - | - | - | -
Power window control | - | × | - | - | - | - | - | - | -
Power window timer | - | × | × | - | - | - | - | - | -
Sunroof control | - | - | × | - | - | - | - | - | -
Sunroof timer | - | × | × | - | - | - | - | - | -
Control of windshield wiper/washer | × | - | - | - | × | - | - | - | -
Rear wiper/washer control | × | - | - | - | × | - | - | - | -
Ignition key cylinder illumination lamp function | - | × | × | - | - | × | - | - | ×
Seat belt warning lamp control | - | × | - | - | - | - | - | - | -
Headlamp control | - | × | - | × | - | - | - | - | -
Tail lamp control | - | × | - | × | - | - | - | - | -
Headlamp automatic shutdown function <except for Australia> | - | × | × | × | - | - | - | - | -
Fog lamp control | - | - | - | × | - | - | - | - | -
Turn-signal lamp control | - | × | - | × | - | - | - | - | -
Room lamp control | - | × | × | - | - | × | × | × | ×
Interior lamp automatic shutdown function | × | - | - | - | - | - | - | - | ×
Door-ajar indicator lamp | - | - | × | - | - | - | × | - | -

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - OPERATION AND FUNCTION QUICK-REFERENCE TABLE FOR INPUT SIGNAL INSPECTION PROCEDURES | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation