[1] PRE-DELIVERY INSPECTION - - AFTER ROAD TEST - 38. AUTOMATIC TRANSMISSION FLUID LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

| 38. AUTOMATIC TRANSMISSION FLUID LEVEL
| Remove the dipstick and check the fluid level. Fluid level is okay if it is in the specified range as illustration at normal engine operating temperature. If the level is below the lower notch, replenish fluid until the level reaches the upper notch. Automatic transmission fluid: DIA QUEEN ATF SP III CAUTION Do not overfill.

[1] PRE-DELIVERY INSPECTION - - AFTER ROAD TEST - 38. AUTOMATIC TRANSMISSION FLUID LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation