[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
Brake reaction plate end play | 0 - 0.16 mm
Low-reverse brake end play | 1.65 - 2.11 mm
Second brake end play | 1.09 - 1.55 mm
Underdrive sun gear end play | 0.25 - 0.45 mm
Input shaft end play | 0.70 - 1.45 mm
Differential case preload | 0.045 - 0.105 mm
Underdrive clutch end play | 1.6 - 1.8 mm
Reverse and overdrive clutch return spring retainer end play | 0 - 0.09 mm
Overdrive clutch end play | 1.6 - 1.8 mm
Reverse clutch end play | 1.2 - 1.4 mm
Direct clutch end play | 1.0 - 1.2 mm
Backlash between differential gear and pinion | 0.025 - 0.150 mm

[23C] AUTOMATIC TRANSMISSION OVERHAUL <W5A5> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation