[51] EXTERIOR - - WIPER AND WASHER - REAR WIPER AND WASHER | PRINT PAGE / INDEX / PRIOR / NEXT

REAR WIPER AND WASHER
WASHER NOZZLE Improved appearance with the washer nozzle inside the high mounted stop lamp.
INTERMITTENT WIPER The rear wiper moves a couple of times at low speed when the switch is turned on (initial continuous movement), and operates at a fixed interval afterwards to provide a clear rear view in rainy weather. The adjusting function also allows setting the intermittent interval at 0, 4, 8 and 16 seconds selectively. The factory setting is 8 seconds interval.
NOTE: The adjusting function allows changing intermittent times of the intermittent wiper (Refer to Group 54B, SWS <Hong Kong spec.> or <Except for Hong Kong spec.> to change the functions).
INTERLOCKED OPERATIONS IN REVERSE When the rear wiper switch is in the intermittent position and the selector lever (gear) in reverse (R), the rear wiper will continuously wipe 2 to 3 times in low speed after about 1 second, and thereafter continue with intermittent wiping with the reverse interlocked wiper function employed.
WIPER ARM AND BLADE Comes with a plastic (resin) wiper arm and blade for lightweightness. The uniformity between the arm and blade was also emphasized for better appearance.
WASHER TANK The washer tank is commonly shared with the windshield washer.
CONSTRUCTION DIAGRAM

[51] EXTERIOR - - WIPER AND WASHER - REAR WIPER AND WASHER | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation