[54A] CHASSIS ELECTRICAL - - HAZARD WARNING LAMP SWITCH - HAZARD WARNING LAMP SWITCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

HAZARD WARNING LAMP SWITCH

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Centre lower panel assembly (Refer to GROUP 52A, Instrument panel assembly <L.H.drive vehicles> or <R.H.drive vehicles>)
|  | 2. | Hazard warning lamp switch

[54A] CHASSIS ELECTRICAL - - HAZARD WARNING LAMP SWITCH - HAZARD WARNING LAMP SWITCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation