[42] BODY - - WINDOW GLASS | PRINT PAGE / INDEX / PRIOR / NEXT

WINDOW GLASS The windshield is laminated glass and the other glass is made of reinforced glass. For some models, the privacy glasses are used for the rear window glasses, quarter window glasses and tailgate window glass <Except vehicles for GCC>. UV-cut glasses are used for the front door window glasses <Vehicles for Hong Kong spec>.
NO. | NAME | TYPE | THICKNESS (mm) | COLOUR | VISIBLE LIGHT PERMEATION RATE (%)
--- | --- | --- | --- | --- | ---
1 | Windshield | Laminated glass | 4.7 | Green | 78.7
2 | Front door window glass <Except vehicles for Hong Kong spec> | Tempered glass | 3.5 | Green | 80.9
Front door window glass <Vehicles for Hong Kong spec> | Green (UV-cut) | 74.6
3 | Rear door window glass | 3.1 | Green | 82.3
Dark grey (privacy glass) | 25
4 | Quarter window glass | 3.1 | Green | 82.3
Dark grey (privacy glass) | 25
5 | Tailgate window glass | 3.1 | Green | 82.3
Dark grey (privacy glass) | 25
6 | Roof lid glass | 4.0 | Dark grey | 18
7 | Roof window glass <Vehicles for Hong Kong spec> | 4.0 | Dark grey | 18
NOTE: The figure at the visible light permeation rate is a reference value. There could be marginal errors.

[42] BODY - - WINDOW GLASS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation