[37] POWER STEERING - - ON-VEHICLE SERVICE - STEERING WHEEL RETURN TO CENTRE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| STEERING WHEEL RETURN TO CENTRE CHECK Conduct a road test: Make both gradual and sudden turns and check the steering wheel return.
| At a vehicle speed of approximately 35 km/h, turn the steering wheel 90°, hold a few seconds, then release. If the steering wheel then returns 70° or more, the return can be judged satisfactory. NOTE: There will be a momentary feeling or "heaviness" when the wheel is turned quickly, but this is not abnormal. (Oil pump discharge amount is especially apt to be insufficient during idling.)

[37] POWER STEERING - - ON-VEHICLE SERVICE - STEERING WHEEL RETURN TO CENTRE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation