[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - TROUBLESHOOTING - INSPECTION PROCEDURE FOR DIAGNOSIS CODES - DTC P0606: Engine-A/T-ECU Main Processor Malfunction | PRINT PAGE / INDEX / PRIOR / NEXT

DTC P0606: Engine-A/T-ECU Main Processor Malfunction
FUNCTION System LSI checks the engine-A/T-ECU for abnormal conditions.
TROUBLE JUDGMENT Check Condition Ignition switch is "ON" position. Judgement Criterion No surveillance pulse signals is input for 0.5 second.
PROBABLE CAUSE Failed the engine-A/T-ECU
| DIAGNOSIS
| STEP 1. Check the trouble symptoms. Q: Does trouble symptom persist? YES: Replace engine-A/T-ECU. NO: Intermittent malfunction (Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points ).

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - TROUBLESHOOTING - INSPECTION PROCEDURE FOR DIAGNOSIS CODES - DTC P0606: Engine-A/T-ECU Main Processor Malfunction | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation