[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - FUEL PUMP RELAY CONTINUITY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| FUEL PUMP RELAY CONTINUITY CHECK
Tester Connection Terminal | Battery Voltage | Normal State
--- | --- | ---
2 - 3 | No Voltage | Continuity
1 - 4 | No Voltage | No continuity
Voltage (Connect positive (+) terminal of battery to terminal No. 3 and negative (-) terminal of battery to terminal No. 2.) | Continuity

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - FUEL PUMP RELAY CONTINUITY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation