[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 26. OPERATION OF SEAT BELTS, SHOULDER BELTS AND RETRACTORS | PRINT PAGE / INDEX / PRIOR / NEXT

| 26. OPERATION OF SEAT BELTS, SHOULDER BELTS AND RETRACTORS
| Verify that the seat belt warning lamp operates properly. Check all seat belts and harnesses to assure that they connect and hold properly. Lean forward to check that the shoulder harnesses allow movement. Check the condition of the belts and anchors. Check for proper seat belt retraction.

[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 26. OPERATION OF SEAT BELTS, SHOULDER BELTS AND RETRACTORS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation