[54A] CHASSIS ELECTRICAL - - COMBINATION METER | PRINT PAGE / INDEX / PRIOR / NEXT

COMBINATION METER The combination meter was designed to enhance the driver's view of the meters and feature an easy-viewing large needle-meter design. At the top centre is the fuel gauge and below it is the water thermometer. To the left is the speedometer and to the right is the tachometer. The speedometer is an electronic type speedometer which operates by the pulse signal generated by the engine-A/T-ECU. The A/T indicator is located at the bottom right and features a LCD* sports mode digital (shift position) display. A large and clear LCD* type odo-trip meter is provided. The odometer continuously displays values while the trip meter adopts a twin-trip (trip A, trip B) function which is switched by a reset button. NOTE: LCD*: Liquid crystal display
CONSTRUCTION DIAGRAM

[54A] CHASSIS ELECTRICAL - - COMBINATION METER | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation