[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - ACCELERATOR PEDAL <4G69-R.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ACCELERATOR PEDAL <4G69-R.H. DRIVE VEHICLES>

REMOVAL AND INSTALLATION CAUTION Never loosen the screw fixing the accelerator pedal assembly resin cover. If the screw is loosened, the sensor incorporated in the resin cover is misaligned and the accelerator pedal position sensor (APS) do not work normally. Do not remove the accelerator pedal pad. If the pad is removed and installed, excessive force may damage APS.
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Accelerator pedal position sensor (APS) connector
|  | 2. | Accelerator pedal assembly
|  | 3. | Accelerator pedal arm stopper

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - ACCELERATOR PEDAL <4G69-R.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation