[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B7. CHECK GEAR OIL LEVEL IN TRANSFER CASE (4WD) | PRINT PAGE / INDEX / PRIOR / NEXT

| B7. CHECK GEAR OIL LEVEL IN TRANSFER CASE (4WD)
| Remove the filler plug of the transfer case.
| Oil level should be at the lower portion of the filler plug hole. Check that the transfer oil is not noticeably dirty, and that it has a suitable viscosity. Tighten the filler plug to the specified torque. Tightening torque: 32 ± 2 N·m

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B7. CHECK GEAR OIL LEVEL IN TRANSFER CASE (4WD) | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation