[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 7: The ignition key can be turned to the LOCK (OFF) position when the selector lever is at a position other than the P position. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 7: The ignition key can be turned to the LOCK (OFF) position when the selector lever is at a position other than the P position.
COMMENTS ON TROUBLE SYMPTOM The cause is probably a malfunction of the key interlock cable or ignition key cylinder lock bar.
Possible causes Malfunction of key interlock cable Malfunction of lock bar
DIAGNOSIS Check by referring to the possible causes.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 7: The ignition key can be turned to the LOCK (OFF) position when the selector lever is at a position other than the P position. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation