[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B10. CHECK GEAR OIL LEVEL IN FRONT AND REAR DIFFERENTIAL | PRINT PAGE / INDEX / PRIOR / NEXT

| B10. CHECK GEAR OIL LEVEL IN FRONT AND REAR DIFFERENTIAL Remove the filler plug.
| Check that the gear oil level is within the specified range from the bottom end of the filler plug hole. If the gear oil level exceeds the standard value, add the specified gear oil up to the bottom end of the filler plug hole. Specified gear oil: Gear oil API classification GL-5 or higher Above 10°C SAE 90 Below 10°C SAE 80W Fit the filler plug and tighten it to the specified torque. Tightening torque: 49 ± 9 N·m

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B10. CHECK GEAR OIL LEVEL IN FRONT AND REAR DIFFERENTIAL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation