[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - VACUUM HOSE - VACUUM HOSE INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

| VACUUM HOSE INSTALLATION When connecting the vacuum hoses, they should be securely inserted onto the nipples. Connect the hoses correctly, using the vacuum hose piping diagram as a guide.

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - VACUUM HOSE - VACUUM HOSE INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation