[36] PARKING BRAKES - - ON-VEHICLE SERVICE - PARKING BRAKE SWITCH CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| PARKING BRAKE SWITCH CHECK
| <L.H. drive vehicles>
| Remove the floor console assembly. (Refer to GROUP 52A, Floor Console Assembly ). Check for continuity between the parking brake switch terminal and the switch mounting bolt.
When parking brake lever is pulled | Less than 2 ohms
When parking brake lever is released | Open circuit
| <R.H. drive vehicles>
| Check for continuity between the parking brake switch terminal and the switch mounting bolt.
When parking brake pedal is depressed | Less than 2 ohms
When parking brake pedal is released | Open circuit

[36] PARKING BRAKES - - ON-VEHICLE SERVICE - PARKING BRAKE SWITCH CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation