[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - ELECTRIC RETRACTABLE REMOTE CONTROLLED DOOR MIRROR - INSPECTION PROCEDURE I-2: Left or right side electric retractable remote controlled door mirror do not work at all. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE I-2: Left or right side electric retractable remote controlled door mirror do not work at all.
| COMMENTS ON TROUBLE SYMPTOM If left or right side electric retractable remote controlled door mirror does not work at all, electric retractable remote controlled door mirror may be defective.
| POSSIBLE CAUSES Malfunction of the electric retractable remote controlled door mirror Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Connector check: C-220 ETACS-ECU connector Q: Is the check result normal? YES: Go to Step 2. NO: Repair the connector.
| Step 2. Connectors check: E-06 remote controlled mirror (LH), E-16 remote controlled mirror (RH) connectors Q: Is the check result normal? YES: Go to Step 3. NO: Repair the connector.
| Step 3. Check the electric retractable remote controlled door mirror. Refer to GROUP 51 - Door mirror . Q: Is the check result normal? YES: Go to Step 4. NO: Replace the electric retractable remote controlled door mirror.
| Step 4. Confirm which door mirror is defective. Q: Confirm which door mirror is defective. LH: Go to Step 5. RH: Go to Step 6.
| Step 5. Check the wiring harness between C-220 ETACS-ECU connector terminal Nos. 31, 40 and E-06 remote controlled mirror (LH) connector terminal Nos. 4, 3. NOTE: Prior to the wiring harness inspection, check intermediate connector C-33, and repair if necessary. Check the input and output signal line for open circuit. Q: Is the check result normal? YES: Go to Step 7. NO: Repair the wiring harness.
| Step 6. Check the wiring harness between C-220 ETACS-ECU connector terminal Nos. 31, 40 and E-16 remote controlled mirror (RH) connector terminal Nos. 4, 3. NOTE: Prior to the wiring harness inspection, check intermediate connector C-30, and repair if necessary. Check the input and output signal line for open circuit. Q: Is the check result normal? YES: Go to Step 7. NO: Repair the wiring harness.
| Step 7. Retest the system. Check that the electric retractable remote controlled mirror works normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - ELECTRIC RETRACTABLE REMOTE CONTROLLED DOOR MIRROR - INSPECTION PROCEDURE I-2: Left or right side electric retractable remote controlled door mirror do not work at all. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation