[54A] CHASSIS ELECTRICAL - - REAR FOG LAMP <2400 for Hong Kong spec. and Argentina> - REAR FOG LAMP TROUBLESHOOTING | PRINT PAGE / INDEX / PRIOR / NEXT

REAR FOG LAMP TROUBLESHOOTING
If the rear fog lamp switch is turned ON when the headlamp or the front fog lamp is turned ON, the rear fog lamp is switched ON and OFF alternatively. If the headlamp and the front fog lamp, the rear fog lamp is turned OFF at the same time. The fog lamps are controlled by the Smart Wiring System (SWS). For Troubleshooting, refer to respective Groups below. Not using SWS monitor <Hong Kong spec.>: GROUP 54B, Troubleshooting . Using SWS monitor <Hong Kong spec.>: GROUP 54C, Troubleshooting . Not using SWS monitor <Except for Hong Kong spec.>: GROUP 54D, Troubleshooting . Using SWS monitor <Except for Hong Kong spec.>: GROUP 54E, Troubleshooting .

[54A] CHASSIS ELECTRICAL - - REAR FOG LAMP <2400 for Hong Kong spec. and Argentina> - REAR FOG LAMP TROUBLESHOOTING | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation