[54A] CHASSIS ELECTRICAL - - HEADLAMP - HEADLAMP LEVELING SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| HEADLAMP LEVELING SWITCH RESISTANCE CHECK
Terminal No. | Switch position | Resistance
--- | --- | ---
4 - 6 | 0 | 750 ohms
1 | 1050 ohms
2 | 1410 ohms
3 | 1710 ohms
4 | 2010 ohms
5 - 6 | 0, 1, 2, 3, 4 | 2830 ohms

[54A] CHASSIS ELECTRICAL - - HEADLAMP - HEADLAMP LEVELING SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation