[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

DIAGNOSIS FUNCTION
DIAGNOSIS CODES CHECK CAUTION Turn off the ignition switch before connecting or disconnecting the MUT-II/III. Connect the MUT-II/III to the diagnosis connector (16-pin) under the instrument under cover, then check diagnosis codes (Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points ).
ERASING DIAGNOSIS CODE CAUTION Turn off the ignition switch before connecting or disconnecting the MUT-II/III. Connect the MUT-II/III to the diagnosis connector and erase the diagnosis code.

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation