[33] FRONT SUSPENSION - - ON-VEHICLE SERVICE - LOWER ARM BALL JOINT AXIAL PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| LOWER ARM BALL JOINT AXIAL PLAY CHECK Raise the vehicle. Remove the stabilizer link from the lower arm. Move the lower arm up and down with your hands to check for an excessive play in the axial direction of the ball joint. If there is an excessive play, replace the lower arm assembly.

[33] FRONT SUSPENSION - - ON-VEHICLE SERVICE - LOWER ARM BALL JOINT AXIAL PLAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation