[54A] CHASSIS ELECTRICAL - - RADIO, TAPE PLAYER, CD PLAYER, SPEAKER, ANTENNA | PRINT PAGE / INDEX / PRIOR / NEXT

RADIO, TAPE PLAYER, CD PLAYER, SPEAKER, ANTENNA
RADIO AND CD PLAYER Two types of 1DIN size integrated audio units are provided for the radio, tape player or CD player.
Item | Type 1 <Vehicles for GCC: standard, Vehicles for General Export (except for Hong Kong spec. and South Africa): option> | Type 2 <Vehicles for Australia and New zealand (2400)>
--- | --- | ---
AM/FM electronic tuning radio | Equipped | Equipped
Tape player | Equipped | -
CD player | - | Equipped
Power amplifier with radio | 25W × 4 | 25W × 4
SPEAKER
Location | Four speakers <Vehicles for General Export (GLS, GLX, 20V model), GCC and Australia and New zealand (LS model)> | Six speakers <Vehicles for Australia and New zealand (XLS, LTD): standard, Vehicles for General Export, GCC, Australia and New zealand (LS model): option>
--- | --- | ---
Front door | - | Equipped (tweeter - 3.5 cm)
Equipped (dual cone full range - 16 cm) | Equipped (full range - 16 cm)
Rear door | Equipped (dual cone full range - 16 cm) | Equipped (full range - 16 cm)
ANTENNA The whip antennas are used. The following two types of antenna are available. Glass antenna <Vehicles for Hong Kong spec.> Whip antenna <Except vehicles for Hong Kong spec.>
CD AUTOCHANGER The model comes standard with a 6 disc CD autochanger of the 1 DIN size. <Standard: Vehicles for Australia and New zealand (XLS, LTD model), Option: Vehicles for General Export (except for Hong Kong spec. and South Africa), GCC (GLS model), Australia and New zealand (LS model)>
CONSTRUCTION DIAGRAM
NOTE: The * indicates equipped on the left and right sides.

[54A] CHASSIS ELECTRICAL - - RADIO, TAPE PLAYER, CD PLAYER, SPEAKER, ANTENNA | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation