[37] POWER STEERING - - STEERING WHEEL - REMOVAL AND INSTALLATION <2000-SOHC AND 2400> | PRINT PAGE / INDEX / PRIOR / NEXT

STEERING WHEEL

REMOVAL AND INSTALLATION <2000-SOHC AND 2400>
WARNING Before removing the steering wheel and air bag module assembly, refer to GROUP 52B, Service Precautions () and Air Bag Module(s) and Clock Spring (). When removing and installing the steering wheel, do not let it bump against the air bag module.
Post-installation Operation Checking Steering Wheel Position with Wheels Straight Ahead
|  |  | Removal steps
--- | --- | --- | ---
<<A>> |  | 1. | Cover
<<B>> |  | 2. | Air bag module assembly
|  | 3. | Steering wheel mounthing nut
<<C>> |  | 4. | Steering wheel
|  | 5. | Sub harness
| REMOVAL SERVICE POINTS
| <<A>> COVER REMOVAL
| Insert special tool ornament remover (MB990784) at the indicated position to remove the cover. NOTE: The special tool can be inserted through the notch behind the area shown.
| <<B>>AIR BAG MODULE ASSEMBLY REMOVAL
| By sliding section A of the clock spring connector shown in the illustration in the arrow direction, disconnect the connector.
| <<C>> STEERING WHEEL REMOVAL
| Use special tool MB990803 to remove the steering wheel.

[37] POWER STEERING - - STEERING WHEEL - REMOVAL AND INSTALLATION <2000-SOHC AND 2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation