[54B] SMART WIRING SYSTEM (SWS) - - ADJUSTMENT FUNCTION <VEHICLES WITH KEYLESS ENTRY SYSTEM (EXCEPT FOR HONG KONG SPEC.)> | PRINT PAGE / INDEX / PRIOR / NEXT

ADJUSTMENT FUNCTION <VEHICLES WITH KEYLESS ENTRY SYSTEM (EXCEPT FOR HONG KONG SPEC.)>
According to the configuration mode entry conditions of the input switch, the following functions can be adjusted. The data on configuration will be memorized even if the battery is removed. Keyless entry system hazard answerback function Power window timer function Vehicle speed-dependent wiper function Headlamp automatic-shutdown function Delayed lamp-off time of the room lamp Interior lamp automatic-shutdown function Initialization of all functions (Returns to initial settings) Conditions for entering the configuration mode Set each switch to the following state. Hazard lamp switch: OFF Diagnosis control: ON (Connect the MUT-II/III or earth pin one of the diagnosis connector.) Key reminder switch: OFF (Insert the ignition key) Ignition switch: "LOCK" (OFF) position Driver's door switch: OFF (driver's door closed) When the windshield washer switch is ON for more than ten seconds, the tone alarm in the ETACS-ECU sounds for three seconds, and the configuration mode will be set. Conditions for exiting the configuration mode Diagnosis control: OFF (Disconnect the MUT-II/III or the earth of Pin one of the diagnosis connector.) Key reminder switch: ON (Remove the ignition key) Ignition switch: Turning to any position other than "LOCK" (OFF) position Driver's door switch: ON (driver's door opened) When three minutes pass without configurations performed When the other warning tone alarm output is generated Configurations of various functions
Function | Configuration procedure
--- | ---
Keyless entry system hazard answerback function | When the lock button of the transmitter is pressed twice continuously within two seconds, the hazard answerback function during the lock state will be switched between available or unavailable. Function available: Tone alarm sounds once. (Initial state) Function not available: Tone alarm sounds twice. When the unlock button of the transmitter is pressed twice continuously within two seconds, the hazard answerback function during the unlock state will be switched between available or unavailable. Function available: Tone alarm sounds once. (Initial state) Function not available: Tone alarm sounds twice.
Power window timer function | When one of the power window main switch turns ON twice within two seconds (however there must be an interval of more than 0.3 seconds,) the power window timer function will be switched between available or unavailable. Function available: Tone alarm sounds twice. (Initial state) Function not available: Tone alarm sounds five times.
Vehicle speed-dependent wiper function | When the windshield wiper mist switch is turned ON for more than two seconds, the vehicle speed-dependent wiper function is switched between available or unavailable. Function available: Tone alarm sounds once. (Initial state) Function not available: Tone alarm sounds twice.
Headlamp automatic-shutdown function | When the passing switch is turned ON for more than two seconds with the auto-lamp switch ON and the turn signal lamp switch turned to RH, the headlamp automatic-shutdown function is switched between available or unavailable. Function not available: Tone alarm sounds twice. Function available: (when the tail lamp illuminates with the ignition switch turned to the "LOCK" (OFF) position, it is not automatically turned off): Tone alarm sounds once. (Initial state)
Delayed lamp-off time of the room lamp | When the turn signal lamp switch is set in the order of RH to LH to RH to LH within three seconds from the LH position, the delayed lamp-off time switches (Returns to a after e, and repeats from a in order.) 30 seconds: Tone alarm sounds once. (Initial state) 10 seconds: Tone alarm sounds twice. 0 seconds (No delay time): Tone alarm sounds three times. 15 seconds: Tone alarm sounds four times. 7.5 seconds: Tone alarm sounds five times.
Interior lamp automatic-shutdown function | When the hazard lamp switch is turned ON for more than two seconds, the interior lamp cut-off function switches in the following order. (a and b switches alternately) Function available: Tone alarm sounds once. (Initial state) Function not available: Tone alarm sounds twice.
Initialization of all functions | When the windshield washer switch is ON for more than 20 seconds continuously, the tone alarm sounds twice, and all functions will be initialized. (Settings are returned to their initial states.) The configuration mode entry tone alarm sounds after 10 seconds, however to initialize all functions, the ON state will continue for 20 seconds. When the windshield washer switch is ON for more than 20 seconds continuously without the configuration mode set, the configuration mode will be set after 10 seconds without the initialization of all functions.

[54B] SMART WIRING SYSTEM (SWS) - - ADJUSTMENT FUNCTION <VEHICLES WITH KEYLESS ENTRY SYSTEM (EXCEPT FOR HONG KONG SPEC.)> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation