[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - RADIO WITH TAPE PLAYER AND CD PLAYER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

RADIO WITH TAPE PLAYER AND CD PLAYER

REMOVAL AND INSTALLATION
|  |  | Radio removal steps
--- | --- | --- | ---
|  | 1. | Centre panel assembly (Refer to GROUP 52A, Instrument panel assembly <L.H.drive vehicles> or <R.H.drive vehicles>)
|  | 2. | Radio bracket
|  | 3. | Box
|  | 4. | Antenna feeder cable and harness connector
|  | 5. | Radio and tape player or radio and CD player
|  | 6. | DIN cable
|  | 7. | CD changer

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - RADIO WITH TAPE PLAYER AND CD PLAYER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation