[42] BODY - - DOOR - DOOR HANDLE AND LATCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

DOOR HANDLE AND LATCH

REMOVAL AND INSTALLATION
Pre-removal Operation Door Trim Assembly Removal (Refer to GROUP 52A, Door Trim ). | Post-installation Operation Door Inside Handle Play Adjustment (Refer to ). Door Outside Handle Play Check (Refer to ). Door Trim Assembly Installation (Refer to GROUP 52A, Door Trim ).
|  |  | Door handle and door latch assembly removal steps
--- | --- | --- | ---
| >>C<< | 1. | Door inside handle
|  | • | Waterproof film (Refer to .)
| >>B<< | 2. | Lower sash
|  | 3. | Door outside handle
|  | 4. | Door lock key cylinder
|  | 5. | Screw
|  | 6. | Door latch assembly
|  | 7. | Inside lock cable <Front door>
|  | 8. | Inside lock rod <Rear door>
|  | 9. | Inside handle rod
|  | 10. | Outside handle rod
|  |  | Door check removal steps
|  | • | Waterproof film (Refer to .)
| >>A<< | 11. | Door check
| INSTALLATION SERVICE POINTS
| >>A<< DOOR CHECK INSTALLATION
| Install the door check so that the identification mark faces upwards.
ITEM | IDENTIFICATION MARK
--- | ---
Front Door | Left door | 39L
Right door | 39R
Rear Door | Left door | 40L
Right door | 40R
| >>B<< LOWER SASH INSTALLATION Insert the lower sash into the window rear sash (at door) securely.
| >>C<< DOOR INSIDE HANDLE INSTALLATION When connecting the inside cable <Front door> or the inside rod <Rear door> to the door inside handle, ensure that the door latch and the inside handle are unlocked.

[42] BODY - - DOOR - DOOR HANDLE AND LATCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation