[34] REAR SUSPENSION - - TRAILING ARM ASSEMBLY - REMOVAL AND INSTALLATION <2WD> | PRINT PAGE / INDEX / PRIOR / NEXT

TRAILING ARM ASSEMBLY

REMOVAL AND INSTALLATION <2WD>
CAUTION * : Indicates parts which should be temporarily tightened, and then fully tightened with the vehicle on the ground in the unladen condition.
Pre-removal Operation Brake Fluid Draining Rear Hub Assembly Removal (Refer to GROUP 27A, Rear Axle Hub Assembly ). | Post-installation Operation Rear Hub Assembly Installation (Refer to GROUP 27A, Rear Axle Hub Assembly ). Brake Fluid Supplying and Bleeding (Refer to GROUP 35A, On-vehicle Service - Bleeding ). Rear Wheel Alignment Check and Adjustment (Refer to ). Parking Brake Pedal Stroke Adjustment (Refer to GROUP 36, On-vehicle Service - Parking Brake Pedal Stroke Check and Adjustment ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Rear ABS Sensor (Refer to GROUP 35B, ABS Sensor ).
|  | 2. | Parking brake cable
|  | 3. | Brake hose and trailing arm connection
|  | 4. | Rear brake assembly
| >>A<< | 5. | Lower arm and stabilizer link connection
|  | 6. | Lower arm and shock absorber connection
|  | 7. | Control link and trailing arm connection
|  | 8. | Upper arm and trailing arm connection
<<A>> |  | 9. | Lower arm and trailing arm connection
|  | 10. | Trailing arm and body connection
|  | 11. | Trailing arm
| REMOVAL SERVICE POINT
| <<A>> LOWER ARM AND TRAILING ARM DISCONNECTION
| After supporting the lower arm with a jack, separate the lower arm and trailing arm connection.
| INSTALLATION SERVICE POINT
| >>A<< STABILIZER LINK INSTALLATION
| Tighten the self-locking nut until the stabilizer link thread part protruding length meets the standard value. Standard value (A): 6 - 8 mm

[34] REAR SUSPENSION - - TRAILING ARM ASSEMBLY - REMOVAL AND INSTALLATION <2WD> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation