[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - ELECTRIC RETRACTABLE REMOTE CONTROLLED DOOR MIRROR - INSPECTION PROCEDURE I-6: Keyless entry system-linked fold/unfold function does not work normally. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE I-6: Keyless entry system-linked fold/unfold function does not work normally.
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| COMMENTS ON TROUBLE SYMPTOM The ETACS-ECU operates this function in accordance with the keyless entry transmitter input signals. If this function does not work normally, keyless entry transmitter input signal circuit or the ETACS-ECU may be defective. In addition, it is possible that the function except the keyless entry system-linked fold/unfold function has been set by using the adjustment function.
| POSSIBLE CAUSES Malfunction of the keyless entry transmitter Malfunction of ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Pulse check Check the input signals from the keyless entry system transmitter switches.
System switch | Check conditions
--- | ---
Keyless entry system transmitter switches | When the switch is turned from off to on
OK: The MUT-II/III sounds or the voltmeter needle fluctuates. Q: Is the check result normal? YES: Go to Step 2. NO: Refer to inspection procedure P-16 "Each switch signal of the keyless entry transmitter is not received."
| Step 2. Check the SWS monitor customized function. Use the SWS monitor customize function to confirm that "WING MIRROR" is set to "KEYLESS LINK". CAUTION The SWS monitor must be used in order to confirm and change that setting. Use the SWS monitor to confirm and/or change the customized function. Q: Is the check result normal? YES: Go to Step 3. NO: Use the SWS monitor customize function to set the "WING MIRROR" to "KEYLESS LINK" (Refer to GROUP 54C - Adjustment function ).
| Step 3. Retest the system. The vehicle speed-dependent unfolding function should now work normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - ELECTRIC RETRACTABLE REMOTE CONTROLLED DOOR MIRROR - INSPECTION PROCEDURE I-6: Keyless entry system-linked fold/unfold function does not work normally. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation