[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - SYMPTOM PROCEDURES - Inspection Procedure 1: When the Brake Pedal is Depressed, Auto-cruise Control is not Cancelled. | PRINT PAGE / INDEX / PRIOR / NEXT

SYMPTOM PROCEDURES

Inspection Procedure 1: When the Brake Pedal is Depressed, Auto-cruise Control is not Cancelled.
COMMENTS ON TROUBLE SYMPTOM The stop lamp switch circuit is suspected.
PROBABLE CAUSES Malfunction of the connector. Malfunction of the harness. Malfunction of the stop lamp switch. Malfunction of the engine-A/T-ECU.
DIAGNOSIS Refer to , Diagnosis Trouble Code Procedures - Code No. 22: Stop lamp switch system.

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - SYMPTOM PROCEDURES - Inspection Procedure 1: When the Brake Pedal is Depressed, Auto-cruise Control is not Cancelled. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation