[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ENGINE-A/T-ECU - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ENGINE-A/T-ECU

REMOVAL AND INSTALLATION
<LH DRIVE VEHICLES> CAUTION Always register the ignition key(s) when the engine-A/T-ECU is replaced (Refer to GROUP 54A, Ignition Switch - On-vehicle Service - How to Register Encrypted Code ) <Vehicles with immobiliser>.
Pre-removal and Post-installation Operation Cowl Side Trim (RH) Removal and Installation (Refer to GROUP 52A, Instrument Panel Assembly ).
|  |  | REMOVAL STEPS
--- | --- | --- | ---
| >>A<< | • | Initialisation procedure (installation only)
|  | 1. | Engine-A/T-ECU connector
|  | 2. | Engine-A/T-ECU
|  | 3. | Engine-A/T-ECU bracket
| INSTALLATION SERVICE POINT
| >>A<< INITIALISATION PROCEDURE Turn the ignition switch on then off, and keep it off for at least 10 seconds.
<RH DRIVE VEHICLES> CAUTION Register the ignition key ID when the engine-A/T-ECU is replaced (Refer to GROUP 54A, Ignition Switch - On-vehicle Service - How to Register Encrypted Code ) <Vehicles with immobiliser>.
Pre-removal and Post-installation Operation Instrument panel console side cover (LH) Removal and Installation (Refer to GROUP 52A, Instrument Panel Assembly ).
|  |  | REMOVAL STEPS
--- | --- | --- | ---
| >>A<< | • | Initialisation procedure (installation only)
|  | 1. | Side cover trim bracket
|  | 2. | Engine-A/T-ECU connector
|  | 3. | Engine-A/T-ECU
|  | 3. | Engine-ECU bracket
| INSTALLATION SERVICE POINT
| >>A<< INITIALISATION PROCEDURE Turn the ignition switch on then off, and keep it off for at least 10 seconds.

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ENGINE-A/T-ECU - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation