[54A] CHASSIS ELECTRICAL - - HEADLAMP - HEADLAMP - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <2400>
Post-installation Operation Headlamp Aiming Adjustment (Refer to ).
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Front bumper assembly (Refer to GROUP 51, Front Bumper Assembly ).
<<A>> |  | 1. | Headlamp assembly
| REMOVAL SERVICE POINT
| <<A>> HEADLAMP ASSEMBLY REMOVAL
| Remove half of the front bumper assembling clips and bolts. NOTE: The figure illustrates the procedures to remove the headlamp assembly (LH). Slide the front bumper down to remove the headlamp assembly.

[54A] CHASSIS ELECTRICAL - - HEADLAMP - HEADLAMP - REMOVAL AND INSTALLATION <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation